(kicad_pcb (version 20171130) (host pcbnew 5.0.2-1.fc29)
  (general
    (thickness 1.6)
    (drawings 13)
    (tracks 52)
    (zones 0)
    (modules 23)
    (nets 15)
  )
  (page A4)
  (layers
    (0 F.Cu signal hide)
    (31 B.Cu signal hide)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 1)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.75 0.55)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(R4-Pad1)")
  (net 2 "Net-(C1-Pad2)")
  (net 3 "Net-(C1-Pad1)")
  (net 4 "Net-(C2-Pad1)")
  (net 5 "Net-(C2-Pad2)")
  (net 6 GND)
  (net 7 "Net-(R6-Pad1)")
  (net 8 "Net-(R8-Pad1)")
  (net 9 VDD)
  (net 10 "Net-(C5-Pad1)")
  (net 11 VEE)
  (net 12 "Net-(C8-Pad1)")
  (net 13 "Net-(J2-Pad4)")
  (net 14 "Net-(U1-Pad7)")
  (net_class Default "Esta es la clase de red por defecto."
    (clearance 0.5)
    (trace_width 1)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net GND)
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(C1-Pad2)")
    (add_net "Net-(C2-Pad1)")
    (add_net "Net-(C2-Pad2)")
    (add_net "Net-(C5-Pad1)")
    (add_net "Net-(C8-Pad1)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R6-Pad1)")
    (add_net "Net-(R8-Pad1)")
    (add_net "Net-(U1-Pad7)")
    (add_net VDD)
    (add_net VEE)
  )
  (net_class Mecago ""
    (clearance 0.4)
    (trace_width 0.4)
    (via_dia 1)
    (via_drill 0.6)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_bornier-4_P5.08mm (layer F.Cu) (tedit 59FF03D1)
    (at 137.16 71.12 90)
    (descr "simple 4-pin terminal block, pitch 5.08mm, revamped version of bornier4")
    (tags "terminal block bornier4")
    (fp_text reference J2 (at 17.145 -5.715 180) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x04 (at 7.6 4.75 90) (layer F.Fab))
    (fp_text user %R (at 7.62 0 90) (layer F.Fab))
    (pad 4 thru_hole circle (at 15.24 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 13 "Net-(J2-Pad4)"))
    (pad 1 thru_hole rect (at 0 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (pad 3 thru_hole circle (at 10.16 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 2 thru_hole circle (at 5.08 0 90) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_bornier-4_P5.08mm.wrl
      (offset (xyz 7.619999885559082 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_SOIC:SO-8_5.3x6.2mm_Pitch1.27mm (layer F.Cu) (tedit 5C548577)
    (at 116.84 64.77)
    (descr "8-Lead Plastic Small Outline, 5.3x6.2mm Body (http://www.ti.com.cn/cn/lit/ds/symlink/tl7705a.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference U1 (at 0 -4.13) (layer F.SilkS))
    (fp_text value NE5532 (at 0 4.13) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 8 smd rect (at 3.7 -1.905) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD))
    (pad 7 smd rect (at 3.7 -0.635) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad7)"))
    (pad 6 smd rect (at 3.7 0.635) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 5 smd rect (at 3.7 1.905) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 4 smd rect (at -3.7 1.905) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 11 VEE))
    (pad 3 smd rect (at -3.7 0.635) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at -3.7 -0.635) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R6-Pad1)"))
    (pad 1 smd rect (at -3.7 -1.905) (size 1.75 0.55) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R8-Pad1)"))
    (model ${KISYS3DMOD}/Housings_SOIC.3dshapes/SO-8_5.3x6.2mm_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 102.87 72.31 90)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -1.7 90) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -1.35 0 90) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 102.87 55.96 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at -3.255 0) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C2-Pad2)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 104.22 67.945 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 108.505 66.04 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 105.41 72.41 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.75 270) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 270) (layer F.Fab))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer F.Cu) (tedit 58AA84A8)
    (at 105.41 55.86 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 3.155 0 180) (layer F.SilkS))
    (fp_text value 2.2u (at 0 1.75 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.75 90) (layer F.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(C2-Pad2)"))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 104.06 59.69 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 108.505 62.865 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0.555 1.905 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 109.22 71.2 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 -1.7 270) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 1 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 111.68 59.69 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 1.825 1.905 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R8-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(R6-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Terminal_Blocks:TerminalBlock_bornier-3_P5.08mm (layer F.Cu) (tedit 59FF03B9)
    (at 96.52 58.42 270)
    (descr "simple 3-pin terminal block, pitch 5.08mm, revamped version of bornier3")
    (tags "terminal block bornier3")
    (fp_text reference J1 (at -3.81 0) (layer F.SilkS))
    (fp_text value Screw_Terminal_01x03 (at 5.08 5.08 270) (layer F.Fab))
    (fp_text user %R (at 5.08 0 270) (layer F.Fab))
    (pad 3 thru_hole circle (at 10.16 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 2 "Net-(C1-Pad2)"))
    (pad 2 thru_hole circle (at 5.08 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 6 GND))
    (pad 1 thru_hole rect (at 0 0 270) (size 3 3) (drill 1.52) (layers *.Cu *.Mask)
      (net 5 "Net-(C2-Pad2)"))
    (model ${KISYS3DMOD}/Terminal_Blocks.3dshapes/TerminalBlock_bornier-3_P5.08mm.wrl
      (offset (xyz 5.079999923706055 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 120.65 59.055 90)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C3 (at 0 -1.25 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 90) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 90) (layer F.Fab))
    (pad 2 smd rect (at 0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -0.95 0 90) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 58AA84FB)
    (at 125.095 64.865 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C4 (at -3.905 0.635) (layer F.SilkS))
    (fp_text value "10u / 25V" (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 58AA84FB)
    (at 130.175 64.77 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C5 (at 0 -2.25 270) (layer F.SilkS))
    (fp_text value "10u / 25V" (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603_HandSoldering (layer F.Cu) (tedit 58AA848B)
    (at 113.665 70.8 270)
    (descr "Capacitor SMD 0603, hand soldering")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C6 (at 0 -1.25 270) (layer F.SilkS))
    (fp_text value 100n (at 0 1.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.25 270) (layer F.Fab))
    (pad 1 smd rect (at -0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 11 VEE))
    (pad 2 smd rect (at 0.95 0 270) (size 1.2 0.75) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 58AA84FB)
    (at 120.015 72.485 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C7 (at 0 -2.25 270) (layer F.SilkS))
    (fp_text value "10u / 25V" (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 11 VEE))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_1210_HandSoldering (layer F.Cu) (tedit 58AA84FB)
    (at 130.175 72.485 270)
    (descr "Capacitor SMD 1210, hand soldering")
    (tags "capacitor 1210")
    (attr smd)
    (fp_text reference C8 (at 0 -2.25 270) (layer F.SilkS))
    (fp_text value "10u / 25V" (at 0 2.5 270) (layer F.Fab))
    (fp_text user %R (at 0 -2.25 270) (layer F.Fab))
    (pad 1 smd rect (at -2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 2 0 270) (size 2 2.5) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_1210.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 114.22 55.88 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 1.825 1.905 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(R8-Pad1)"))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(J2-Pad4)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 128.825 59.69 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at -0.08 1.905 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 9 VDD))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(C5-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 58E0A804)
    (at 125.015 70.485 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 -1.7 180) (layer F.SilkS))
    (fp_text value 100 (at 0 1.75 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(C8-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 11 VEE))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23 (layer F.Cu) (tedit 5A02FF57)
    (at 103.235 64.455 180)
    (descr "SOT-23, Standard")
    (tags SOT-23)
    (attr smd)
    (fp_text reference D1 (at 0 -2.5 180) (layer F.SilkS))
    (fp_text value NUP2105L (at 0 2.5 180) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd rect (at -1 -0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at -1 0.95 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(C2-Pad1)"))
    (pad 3 smd rect (at 1 0 180) (size 0.9 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 GND))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text "NE5532 PREAMP (2.2019)" (at 116.205 78.74) (layer F.SilkS))
  (gr_circle (center 138.43 77.47) (end 140.18 77.47) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 138.43 49.53) (end 140.18 49.53) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 95.25 77.47) (end 97 77.47) (layer Edge.Cuts) (width 0.15))
  (gr_circle (center 95.25 49.53) (end 97 49.53) (layer Edge.Cuts) (width 0.2))
  (gr_line (start 91.44 81.28) (end 91.44 45.72) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 81.28) (end 91.44 81.28) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 142.24 45.72) (end 142.24 81.28) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 91.44 45.72) (end 142.24 45.72) (layer Edge.Cuts) (width 0.15))
  (zone (net 6) (net_name GND) (layer F.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.075 46.355) (xy 92.075 80.645) (xy 141.605 80.645) (xy 141.605 46.355)
      )
    )
  )
  (zone (net 6) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 92.075 46.355) (xy 92.075 80.645) (xy 141.605 80.645) (xy 141.605 46.355)
      )
    )
  )
)
